Replicated design from: <http://www.vatsaas.org/RTV/Support/relay/launcher.aspx>

Controller 4-pin RJ11 connector:

Yellow - Launch (4)

Black - Continuity (1)

Green - Ground (3)

Red - Return (2)

\*pin out looking at male plug from left to right 1-4, pins on top

\*pins and colors are flipped for the launcher

Relay 1

Black - GND

White - Inductor

Blue - N.C.

Green - N.O.